I-O steady state characteristics (Figures 5(c))

* Open IOPAincreasing.m and IOPAdecreasing.m and set the parameter values and Initial Conditions according to the figure caption.
* Open IOsscharacteristicsPosAuto.m and set the values of mu prime, of the maximum value of the input and of px according to the figure.
* Run IOsscharacteristicsPosAuto.m